{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Przedmiar (zam podst)"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Przedmiar (zam podst)","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[[16,0,16,4],[17,0,17,4]],"flags":["formulas_cached_only"]}
[{"$nulls":4},"Załącznik numer 7 do SIWZ"]
[]
[null," KOSZTORYS OFERTOWY"]
[null,"Nazwa zadania - Bieżące utrzymanie dróg gminnych "]
[]
[]
["Adres inwestycji - drogi na terenie gminy Mikołajki"]
["Inwestor - Gmina Mikołajki"]
["Adres inwestora - ul. Kolejowa 7, 11-730 Mikołajki"]
["Branża: Drogowa "]
[]
["L.p","Opis robót","Jm","Ilość","Cena jednostkowa netto","Wartość                                      netto"]
[1,"Równanie i profilowanie dróg o nawierzchni szutrowej – średnia szerokość 4 m","m2",200000]
[2,"Uzupełnienie ubytków na drogach o nawierzchni szutrowej kruszywem naturalnym wraz z zagęszczeniem mechanicznym ","t",2500]
[3,"Uzupełnienie ubytków na drogach o nawierzchni szutrowej kruszywem C50/30 wraz z zagęszczeniem ","t",1200]
[4,"Odtworzenie, odmulenie rowów przydrożnych z wywozem ziemi ","mb",4300]
["RAZEM NETTO: "]
["RAZEM BRUTTO: "]