{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Arkusz1","Arkusz2","Arkusz3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Arkusz1","index":0,"n_rows":85,"n_cols":8,"rows_kept":85,"cut":false,"hidden":false,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,7],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,4,5],[4,6,5,6],[4,7,5,7],[7,2,7,7],[13,4,13,7],[14,2,14,7],[24,4,24,7],[25,2,25,7],[49,4,49,7],[50,3,50,6],[51,3,51,6],[34,5,34,7],[52,3,52,6],[58,0,60,0],[58,3,60,3],[58,4,60,4],[58,5,60,5],[58,6,60,6],[57,0,57,3],[56,0,56,4]],"flags":["formulas_cached_only"]}
["FORMULARZ 1.0"]
["KOSZTORYS OFERTOWY - roboty drogowe "]
["Budowa wielofunkcyjnego, szutrowego toru wyścigowego, narciarskiego i biegowego"]
[]
["Lp.","Kod pozycji","Numer SST","Nazwa i opis pozycji","Jednostka",null,"Cena jedn.","Wartość"]
[{"$nulls":4},"Nazwa","Ilość"]
[1,2,3,"4",5,6,7,8]
[null,null,"DZIAŁ OGÓLNY"]
["*",null,"DM.00.00.00","WYMAGANIA OGÓLNE","___"]
[1,null,null,"-koszt dostosowania się do Wymagań Ogólnych zawartych w Specyfikacji Technicznej DM 00.00.00","-","-","ryczałt"]
[2,null,null,"-wybudowanie objazdów /przejazdów i organizacja ruchu","-","-","ryczałt"]
[3,null,null,"-utrzymanie objazdów/przejazdów i organizacja ruchu","-","-","ryczałt"]
[4,null,null,"-likwidacja objazdów/przejazdów i organizacja ruchu","-","-","ryczałt"]
["*",null,null,"SUMA CZĘŚCIOWA"]
[null,45100000,"PRZYGOTOWANIE TERENU POD BUDOWĘ"]
["*",null,"D.01.00.00","ROBOTY PRZYGOTOWAWCZE","___"]
["*",null,"D.01.01.01","Odtworzenie trasy i punktów wysokościowych w terenie równinnym","___"]
[5,null,null,"- tor  i droga serwisowa","km",3.38]
[null,null,null,"- parkingi","ha",0.67]
["*",null,"D.01.02.02","Zdjęcie warstwy humusu","___"]
[6,null,null,"- zdjęcie warstwy humusu grub. 10 cm","m2",36528]
["*",45111000,"D.02.00.00.","ROBOTY ZIEMNE","___"]
["*",null,"D.02.01.01","Wykonanie wykopów w gruntach I - V kat.","___"]
[7,null,null,"- wykonanie wykopów w gruncie kat. I-IV z przemieszczeniem na nasyp lub odkład","m3",22223]
["*",null,null,"SUMA CZĘŚCIOWA"]
[null,45000000,"ROBOTY BUDOWLANE"]
["*",45233000,"D.04.00.00","PODBUDOWY","___"]
["*",null,"D.04.01.01.","Koryto wraz z profilowaniem i zagęszczaniem podłoża","___"]
[8,null,null,"- profilowanie i zagęszczanie podłoża pod warstwy konstrukcyjne","m2",27350]
["*",null,"D.04.04.01","Podbudowa z kruszywa naturalnego","___"]
[9,null,null,"- warstwa podbudowy z pospółki gr. 10cm","m2",10590]
["*",45233000,"D.05.00.00","NAWIERZCHNIE","___"]
["*",null,"D.05.01.03","Nawierzchnia z kruszywa łamanego gr. 15cm","___"]
[10,null,null,"-nawierzchnia drogi serwisowej                                                                 ","m2",3620]
[11,null,null,"-nawierzchnia parkingów                                                                 ","m2","NIE BĘDZIE REALIZOWANA W RAMACH ZAMÓWIENIA"]
["*",null,"D.05.03.101","Nawierzchnia z gruntu stabilizowanego spoiwem hydraulicznym","___"]
[12,null,null,"- nawierzchnia toru","m2",16760]
["*",null,"D.05.03.101","Skropienie emulsją asfaltową szybkorozpadową lub asfaltem upłynnionym w ilości 1.2kg/m2 i posypanie grysem frakcji 2-8 mm w ilości 2.5kg/m2","___"]
[13,null,null,"- nawierzchnia toru","m2",16760]
["*",null,"D.06.00.00","ROBOTY WYKOŃCZENIOWE","___"]
["*",null,"D.06.02.01","Przepusty pod zjazdami","___"]
[14,null,null,"- wykonanie przepustów betonowych fi 400 - 6 sztuk","m",63]
["*",null,"D.07.00.00","URZĄDZENIA BEZPIECZEŃSTWA RUCHU","___"]
["*",null,"D.07.05.01","Bariery ochronne stalowe","___"]
[15,null,null,"- ustawienie barier ochronnych SP-09 z podwójnym licem beriery","mb",1233]
[16,null,null,"- ustawienie barier ochronnych SP-10 z podwójnym licem beriery","mb",984]
["*",null,"GG.00.12.01","Pomiar powykonawczy zrealizowanych obiektów drogowych","___"]
[17,null,null,"- tor  i droga serwisowa","km",3.38]
[18,null,null,"- parkingi","ha",0.67]
["*",null,null,"SUMA CZĘŚCIOWA"]
[null,null,null,"RAZEM CENA OFERTOWA NETTO"]
[null,null,null,"PODATEK VAT 22%"]
[null,null,null,"RAZEM CENA OFERTOWA BRUTTO"]
[]
[]
[]
["KOSZTORYS OFERTOWY"]
["roboty mostowe"]
["LP.","Pozycja","Wyszczególnienie","Jedn. miary","Ilość","Cena jedn.[zł]","Wartość [zł]"]
[null,"specyfik.","elementów"]
[null,"technicz.","rozliczeniowych"]
[1,2,4,5,6,7,8]
[0,"D.03.02.02","PRZEPUST km 0+980,10","X","X","X","X"]
[0,0,"ROBOTY ZIEMNE","x","x","x","x"]
[1,0,"Wykonanie podsypki pod przepustem / Nasypy wraz z wykonaniem stożków","m3",1797.1]
[2,0,"Tłuczeń","m3",78]
[3,0,"Chudy beton","m3",23.8]
[0,0,"GEOKOMPOZYTY","x","x"]
[4,0,"Geotkanina","m2",390]
[5,0,"Geomembrana","m2",118]
[6,0,"Geowłóknina filtracyjna","m2",237]
[0,0,"INNE ROBOTY","x","x"]
[7,0,"Umocnienie nasypów - obrukowanie kamieniem naturlnym gr.10cm","m2",301.9]
[8,0,"Umocnienie nasypów - elementy drobnowymiarowe typu polbruk","m2",46.2]
[9,0,"Rura stalowa ocynk. spiralnie karbowana z powłoką epoksydową VBH15","mb",24,null,"dostawa i montaż po stronie zamawiającego "]
[10,0,"Schody skarpowe (detal mostowy SCH01)","mb",17.7]
[11,0,"Ciek skarpowy","mb",17.7]
[12,0,"Balustrada (detal mostowy BAL6)","mb",53.6]
[13,0,"Dren podłużny","mb",38]
[14,0,"Bariera betonowa jednostronna","mb",60]
[]
[null,"Razem budowa przepustu netto"]
[null,"ŁĄCZNIE BUDOWA PRZEPUSTU NETTO:"]
[null,"VAT    22%"]
[null,"ŁĄCZNIE BUDOWA PRZEPUSTU BRUTTO:"]

{"sheet":"Arkusz2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Arkusz3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}